
            D-Link DHN-520 10Mb Home Phoneline NIC Installation
                            for Windows 98

 Getting Started
 ---------------

    The Windows 98 installation disks or CD are need to complete this
    install.

    Windows 98 Installation Procedure
    ---------------------------------

     1. Make sure your computer is power-off.

     2. Plug the adapter into one PCI slot of your computer.

     3. Turn on the power. Your computer should be booting.

     4. Windows 98 will find new hardware, and
        "Add New Hardware Wizard" will appear.

     5. Insert the driver diskette into the floppy disk, and
        press "Next", and "Next" again in the following window.

     6. Select "Specify a location" in the checkbox, and press "Next"
        to continue. specify the path (D:\), if use CD. (D: is CD drive)
        (A:\), if use floppy disk.

     7. The wizard should found the driver now. Follow the direction
        to complete installation.

     8. After finishing the installation, the Windows system will ask
        you to restart the system. Select "YES" to reboot.


 Trouble Shooting
 ----------------

     - Everything is OK in Device Manager, but network adapter still
       does't function properly. Please make sure that your Computer
       name is different from others in the same network.  You can change
       your Computer name in

       "My Computer" -> "Control Panel" -> "Network" -> "Identification"
       icons
