
          D-Link DHN-520 10Mb Home Phoneline NIC Installation
                            for Windows 2000

 Getting Started
 ---------------

    The Windows 2000 installation CD is needed to complete this
    installation.

    Windows 2000 Installation Procedure
    -----------------------------------

     1. Make sure your computer is power-off.

     2. Plug the adapter into one PCI slot of your computer.

     3. Turn on the power. Your computer should be booting.

     4. Windows 2000 will find new hardware, and
        "Found New Hardware Wizard" will appear.

     5. Insert the driver diskette into the floppy disk, and
        press "Next", and "Next" again in the following windows.

     6. Select "Specify a location" in the checkbox, and press "Next"
        to continue.

     7. In the following dialog box, specify the directory of the driver
        files. For example:

            A:\  (A: is floppy drive)
                        OR
            D:\  (D: is CD drive)

        and then click "OK".

     8. The wizard should found the driver now. Follow the direction
        to complete installation.

        Notes: Press "Yes" to continue installation when Digital Signature
               Not Found appear.

     9. After finishing the installation, there should be a new
        'Local Area Connection' will appear and the LAN card should works now.


 Trouble Shooting
 ----------------

     - Everything is OK in Device Manager, but network adapter still
       does't function properly. Please make sure that your Computer
       name is different from others in the same network.  You can change
       your Computer name in

       "My Computer" -> "Control Panel" -> "System"
       -> "Network Identification" -> Properties
